,Wattage Comments##OTHER##,WIDTH##LENGTH##MILLIMETERS,WEIGHT##MASS##KILOGRAMS,WATTAGE##ELECTRICAL_WATTAGE##WATTS,VOLTAGE RANGE V##OTHER##,VOLTAGE COMMENTS##OTHER##,VOLTAGE##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,TECHNICAL SHEET##OTHER##,STRUCTURE MATERIAL##OTHER##,RADIUS##LENGTH##MILLIMETERS,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,LIGHTING MATERIAL##OTHER##,HEIGHT##LENGTH##MILLIMETERS,FREQUENCY RANGE Hz##OTHER##,OPTIC_DIAM-134_UPWARD LIGHT##OTHER##,OPTIC_DIAM-134_DOWNWARD LIGHT##OTHER##,E04250##OTHER##,OPTIC_DIAM-70_UPWARD LIGHT##OTHER##,E04240##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,OPTIC_DIAM-70_DOWNARD LIGHT##OTHER##,DIAMETER##LENGTH##MILLIMETERS,DEPTH##LENGTH##MILLIMETERS,COLOR RENDERING INDEX##OTHER##,COLLECTION##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,AVAILABLE FINISHES##OTHER##,ASSEMBLY SHEET##OTHER##,ACCESSORY CODE##OTHER##,ACCESSORIES##OTHER##
Ø70_H465_Direct-IndirectLight_Black_COB-LED_12W_2700K_702lm_45°,2x12W,70.000000000000,2.000000000000,24.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-wall,LUCEPLAN_ALUMINIUM_MATT-BLACK,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-adjustable-extruded-aluminium-wall-lamp-e04-wall-lamp_349375,1E0400240001+1E040/1M0000 (X2),E04240+E041M(x2),Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,465.000000000000,50/60Hz,0,0,0,1,1,Wall fixtures for indoor use. The cylindrical body connects smoothly to architectural surfaces. The optics permit a wide range of lighting solutions for multiple contexts.,0.000000000000,1,70.000000000000,108.000000000000,90,E04 WALL,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_wall-1574157151.pdf,,
Ø134_H465_Direct-IndirectLight_Black_COB-LED_19W_2700K_1030lm_45°,2x19W,134.000000000000,4.000000000000,38.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-wall,LUCEPLAN_ALUMINIUM_MATT-BLACK,67.000000000000,https://www.archiproducts.com/en/products/luceplan/led-adjustable-extruded-aluminium-wall-lamp-e04-wall-lamp_349375,1E0400250001+1E040/2M0000 (X2),E04250+E042M(x2),Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,465.000000000000,50/60Hz,1,1,1,0,0,Wall fixtures for indoor use. The cylindrical body connects smoothly to architectural surfaces. The optics permit a wide range of lighting solutions for multiple contexts.,0.000000000000,0,134.000000000000,168.000000000000,90,E04 WALL,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_wall-1574157151.pdf,,
